02. MaxiAEC - 02. Auto Grids

Page / - last modified by MaxiBIM Admin on 2021/07/01 21:10

02. Auto Grids

last modified by MaxiBIM Admin

on 2021/07/01 21:10

Table of Contents

Auto Grids

1. About this function

Read gridlines in your linked CAD drawing to create Revit Grids with your family and style.

2. Demonstration

3. To use this function:

First, go to the Linked CAD file in plan view and click "Auto Grid".

You can find two columns of layers in the Pop-up window. MaxiAEC allows you to extract drawing lines in CAD file for different grid parts.

To read the grid line layer in the drawing, click the Extract Button and pick a grid line. That layer will be recognised as grid line.

Do the same for Grid headers and annotations. You can view the extracted layers for different elements before creation.

You can also choose between different grid header types, and decide whether you need dimensions between grids

Start the creation, and you can see the created grids in your Revit project.

Related Topics:

Next Topic: Auto Column

Learn more about MaxiBIM common tools, which provides multiple gadgets for your everyday Revit tasks.