02. MaxiAEC - 02. Auto Grids 

Page / - last modified by MaxiBIM Admin on 2021/07/01 21:10 

02. Auto Grids 
last modified by MaxiBIM Admin
on 2021/07/01 21:10

Table of Contents

Auto Grids
1. About this function
•	Read gridlines in your linked CAD drawing to create Revit Grids with your family and style.

2. Demonstration

3. To use this function:
•	First, go to the Linked CAD file in plan view and click "Auto Grid".

•	You can find two columns of layers in the Pop-up window. MaxiAEC allows you to extract drawing lines in CAD file for different grid parts. 

•	To read the grid line layer in the drawing, click the Extract Button and pick a grid line. That layer will be recognised as grid line.

•	Do the same for Grid headers and annotations.  You can view the extracted layers for different elements before creation.

•	You can also choose between different grid header types, and decide whether you need dimensions between grids

•	Start the creation, and you can see the created grids in your Revit project.

Related Topics:
Next Topic: Auto Column
Learn more about MaxiBIM common tools, which provides multiple gadgets for your everyday Revit tasks.